**Canon 77D Kit Lens 1855 IS STM**

The camera has a maximum burst speed and superior buffer depth. The 77D is equipped with a 24.2MP APS-C CMOS sensor. It is featuring an optical viewfinder with a 45-point all cross-type AF system 1. The camera is offering fast, accurate dual pixel CMOS AF with phase detection. The DIGIC 7 Image Processor powers the 77D camera with high image quality and fast operation. The 77D can record in an HDR mode. This mode records video at 1920×1080 in 60p and merges every two frames together into a single one that is of 30p. The camera is tuned with a 7560-pixel RGB+IR metering sensor to ensure accurate exposure and color detection AF. 77D maintains ISO sensitive range of 100 up to a maximum of ISO 25,600 thus it can be expanded up a full stop to ISO 51,200.